(footprint "Filter_3030-6_3x3mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "3x3mm SAW Filter")
	(property "Reference" "REF**"
		(at 0.75 3 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "213d894d-6ec2-4fab-97dd-736e6b6bb77f")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "Untitled"
		(at 0 1 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "7376e2db-fb7a-44c1-8a2d-a373d6cf2f7e")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "32d85f8e-cc8e-4372-ac73-45070c8048cf")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "0130f194-5e66-4295-bc36-1da1720427fc")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_rect
		(start -1.75 -1.75)
		(end 1.75 1.75)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill no)
		(layer "F.SilkS")
		(uuid "be0a00ae-2de0-4b4a-bb28-5476d17cf852")
	)
	(fp_poly
		(pts
			(xy -1.9 1.925) (xy -1.9 2.205) (xy -2.18 1.925) (xy -1.9 1.925)
		)
		(stroke
			(width 0.12)
			(type solid)
		)
		(fill yes)
		(layer "F.SilkS")
		(uuid "e25390ab-15f0-4b7a-8398-1f2cbc79c8ce")
	)
	(fp_rect
		(start -2 -2)
		(end 2 2)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "1b9282b5-6bf1-4cdd-8a69-cae292b76c49")
	)
	(fp_text user "${REFERENCE}"
		(at 0 2.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "d3425d63-7a98-4398-876a-2f0467c12bf6")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd roundrect
		(at -1.195 0.745)
		(size 0.81 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "b12f8af5-6efb-483e-b775-ab69528471fb")
	)
	(pad "2" smd roundrect
		(at 0 1.07)
		(size 0.81 1.05)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "9ad8c276-4ac4-4f26-a30d-d3cd27d002ad")
	)
	(pad "3" smd roundrect
		(at 1.195 1.07)
		(size 0.81 1.05)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "e9e658b7-e92d-48ac-9e8a-4c4b1122253d")
	)
	(pad "4" smd roundrect
		(at 1.195 -1.07)
		(size 0.81 1.05)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "9d58f9fb-3d20-4d8c-b20d-a0dae3e99ebc")
	)
	(pad "5" smd roundrect
		(at 0 -1.07)
		(size 0.81 1.05)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "f2ffa158-ca34-4486-9f9c-2bfa47b1c1f1")
	)
	(pad "6" smd roundrect
		(at -1.195 -1.07)
		(size 0.81 1.05)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "3e3421ba-9e71-4915-8f09-411d4411067c")
	)
	(embedded_fonts no)
	(model "${KIPRJMOD}/shapes3d/User Library-TA0676A SAW Filter 1592_5MHz SMD.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 -0 90)
		)
	)
)
