(export (version D)
  (design
    (source "/home/ktims/infinity/My Documents/electronics/orangepi-neo-gps/orangepi-neo-gps.sch")
    (date "Wed 04 Mar 2020 01:56:03 AM PST")
    (tool "Eeschema 5.1.5")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source orangepi-neo-gps.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref U3)
      (value NEO-M8T)
      (footprint RF_GPS:ublox_NEO)
      (datasheet https://www.u-blox.com/sites/default/files/NEO-LEA-M8T-FW3_DataSheet_%28UBX-15025193%29.pdf)
      (libsource (lib RF_GPS) (part NEO-M8T) (description "GNSS Module NEO M8, VCC 2.7V to 3.6V"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E5DDE90))
    (comp (ref J5)
      (value USB_B_Micro)
      (footprint Connector_USB:USB_Micro-B_Amphenol_10103594-0001LF_Horizontal)
      (datasheet ~)
      (libsource (lib Connector) (part USB_B_Micro) (description "USB Micro Type B connector"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E5DF0DE))
    (comp (ref U4)
      (value TLV1117-33)
      (footprint Package_TO_SOT_SMD:SOT-223-3_TabPin2)
      (datasheet http://www.ti.com/lit/ds/symlink/tlv1117.pdf)
      (libsource (lib Regulator_Linear) (part TLV1117-33) (description "800mA Low-Dropout Linear Regulator, 3.3V fixed output, TO-220/TO-252/TO-263/SOT-223"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E5E090B))
    (comp (ref U1)
      (value DS18B20U)
      (footprint Package_SO:MSOP-8_3x3mm_P0.65mm)
      (datasheet http://datasheets.maximintegrated.com/en/ds/DS18B20.pdf)
      (libsource (lib Sensor_Temperature) (part DS18B20U) (description "Programmable Resolution 1-Wire Digital Thermometer MSOP-8"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E5E1F2D))
    (comp (ref J1)
      (value OPI)
      (footprint Connector_PinSocket_2.54mm:PinSocket_2x20_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_02x20_Odd_Even) (description "Generic connector, double row, 02x20, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E5E2DF4))
    (comp (ref J6)
      (value ANT)
      (footprint Connector_Coaxial:SMA_Molex_73251-1153_EdgeMount_Horizontal)
      (datasheet " ~")
      (libsource (lib Connector) (part Conn_Coaxial) (description "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, ...)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E5E46D8))
    (comp (ref D1)
      (value 1N4148W)
      (footprint Diode_SMD:D_SOD-123)
      (datasheet ~)
      (libsource (lib Diode) (part 1N4148W) (description "75V 0.15A Fast Switching Diode, SOD-123"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E5E8593))
    (comp (ref U2)
      (value TLV1117-33)
      (footprint Package_TO_SOT_SMD:SOT-223-3_TabPin2)
      (datasheet http://www.ti.com/lit/ds/symlink/tlv1117.pdf)
      (libsource (lib Regulator_Linear) (part TLV1117-33) (description "800mA Low-Dropout Linear Regulator, 3.3V fixed output, TO-220/TO-252/TO-263/SOT-223"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E5E982C))
    (comp (ref BT1)
      (value Battery_Cell)
      (footprint Battery:BatteryHolder_Keystone_1060_1x2032)
      (datasheet ~)
      (libsource (lib Device) (part Battery_Cell) (description "Single-cell battery"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E5EB5F7))
    (comp (ref C2)
      (value 10u)
      (footprint Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E5EE97E))
    (comp (ref C1)
      (value 10u)
      (footprint Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E5EF91B))
    (comp (ref R1)
      (value 1)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E5F11A2))
    (comp (ref C5)
      (value 10u)
      (footprint Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E5F2FD7))
    (comp (ref R6)
      (value 1)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E5F423E))
    (comp (ref C4)
      (value 10u)
      (footprint Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E5F5541))
    (comp (ref R5)
      (value 100k)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E62DA99))
    (comp (ref R3)
      (value 27)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E634B2C))
    (comp (ref R4)
      (value 27)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E634BE0))
    (comp (ref SW1)
      (value RESET)
      (footprint Button_Switch_SMD:SW_Push_1P1T_NO_6x6mm_H9.5mm)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push) (description "Push button switch, generic, two pins"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E638AC8))
    (comp (ref R2)
      (value 10)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E641C8F))
    (comp (ref L1)
      (value 27n)
      (footprint Inductor_SMD:L_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part L) (description Inductor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E6424CB))
    (comp (ref C3)
      (value 10n)
      (footprint Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E64590E))
    (comp (ref J3)
      (value BIAS_SEL)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x03) (description "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E64DD41))
    (comp (ref J4)
      (value EXT_BIAS)
      (footprint Connector_Molex:Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x02) (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E65B378))
    (comp (ref H1)
      (value MountingHole)
      (footprint MountingHole:MountingHole_3.2mm_M3_ISO7380_Pad)
      (datasheet ~)
      (libsource (lib Mechanical) (part MountingHole) (description "Mounting Hole without connection"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E661FC5))
    (comp (ref H2)
      (value MountingHole)
      (footprint MountingHole:MountingHole_3.2mm_M3_ISO7380_Pad)
      (datasheet ~)
      (libsource (lib Mechanical) (part MountingHole) (description "Mounting Hole without connection"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E663D17))
    (comp (ref H3)
      (value MountingHole)
      (footprint MountingHole:MountingHole_3.2mm_M3_ISO7380_Pad)
      (datasheet ~)
      (libsource (lib Mechanical) (part MountingHole) (description "Mounting Hole without connection"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E664131))
    (comp (ref H4)
      (value MountingHole)
      (footprint MountingHole:MountingHole_3.2mm_M3_ISO7380_Pad)
      (datasheet ~)
      (libsource (lib Mechanical) (part MountingHole) (description "Mounting Hole without connection"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E664322))
    (comp (ref J2)
      (value OUT_SEL)
      (footprint Connector_PinHeader_2.54mm:PinHeader_2x05_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_02x05_Odd_Even) (description "Generic connector, double row, 02x05, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E674609))
    (comp (ref C6)
      (value 100n)
      (footprint Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E768B2D)))
  (libparts
    (libpart (lib Connector) (part Conn_Coaxial)
      (description "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, ...)")
      (docs " ~")
      (footprints
        (fp *BNC*)
        (fp *SMA*)
        (fp *SMB*)
        (fp *SMC*)
        (fp *Cinch*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_Coaxial))
      (pins
        (pin (num 1) (name In) (type passive))
        (pin (num 2) (name Ext) (type passive))))
    (libpart (lib Connector) (part USB_B_Micro)
      (aliases
        (alias USB_B_Mini))
      (description "USB Micro Type B connector")
      (docs ~)
      (footprints
        (fp USB*))
      (fields
        (field (name Reference) J)
        (field (name Value) USB_B_Micro))
      (pins
        (pin (num 1) (name VBUS) (type power_out))
        (pin (num 2) (name D-) (type passive))
        (pin (num 3) (name D+) (type passive))
        (pin (num 4) (name ID) (type passive))
        (pin (num 5) (name GND) (type power_out))
        (pin (num 6) (name Shield) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_01x02)
      (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x02))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_01x03)
      (description "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x03))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_02x05_Odd_Even)
      (description "Generic connector, double row, 02x05, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_2x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_02x05_Odd_Even))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))
        (pin (num 9) (name Pin_9) (type passive))
        (pin (num 10) (name Pin_10) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_02x20_Odd_Even)
      (description "Generic connector, double row, 02x20, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_2x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_02x20_Odd_Even))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))
        (pin (num 9) (name Pin_9) (type passive))
        (pin (num 10) (name Pin_10) (type passive))
        (pin (num 11) (name Pin_11) (type passive))
        (pin (num 12) (name Pin_12) (type passive))
        (pin (num 13) (name Pin_13) (type passive))
        (pin (num 14) (name Pin_14) (type passive))
        (pin (num 15) (name Pin_15) (type passive))
        (pin (num 16) (name Pin_16) (type passive))
        (pin (num 17) (name Pin_17) (type passive))
        (pin (num 18) (name Pin_18) (type passive))
        (pin (num 19) (name Pin_19) (type passive))
        (pin (num 20) (name Pin_20) (type passive))
        (pin (num 21) (name Pin_21) (type passive))
        (pin (num 22) (name Pin_22) (type passive))
        (pin (num 23) (name Pin_23) (type passive))
        (pin (num 24) (name Pin_24) (type passive))
        (pin (num 25) (name Pin_25) (type passive))
        (pin (num 26) (name Pin_26) (type passive))
        (pin (num 27) (name Pin_27) (type passive))
        (pin (num 28) (name Pin_28) (type passive))
        (pin (num 29) (name Pin_29) (type passive))
        (pin (num 30) (name Pin_30) (type passive))
        (pin (num 31) (name Pin_31) (type passive))
        (pin (num 32) (name Pin_32) (type passive))
        (pin (num 33) (name Pin_33) (type passive))
        (pin (num 34) (name Pin_34) (type passive))
        (pin (num 35) (name Pin_35) (type passive))
        (pin (num 36) (name Pin_36) (type passive))
        (pin (num 37) (name Pin_37) (type passive))
        (pin (num 38) (name Pin_38) (type passive))
        (pin (num 39) (name Pin_39) (type passive))
        (pin (num 40) (name Pin_40) (type passive))))
    (libpart (lib Device) (part Battery_Cell)
      (description "Single-cell battery")
      (docs ~)
      (fields
        (field (name Reference) BT)
        (field (name Value) Battery_Cell))
      (pins
        (pin (num 1) (name +) (type passive))
        (pin (num 2) (name -) (type passive))))
    (libpart (lib Device) (part C)
      (description "Unpolarized capacitor")
      (docs ~)
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part L)
      (description Inductor)
      (docs ~)
      (footprints
        (fp Choke_*)
        (fp *Coil*)
        (fp Inductor_*)
        (fp L_*))
      (fields
        (field (name Reference) L)
        (field (name Value) L))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib Device) (part R)
      (description Resistor)
      (docs ~)
      (footprints
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Diode) (part MMSD914)
      (aliases
        (alias 1N4148W)
        (alias BAV16W)
        (alias 1N4448W)
        (alias MMSD4148))
      (description "100V 0.2A Switching Diode, SOD-123")
      (docs https://www.onsemi.com/pub/Collateral/MMSD914T1-D.PDF)
      (footprints
        (fp D*SOD?123*))
      (fields
        (field (name Reference) D)
        (field (name Value) MMSD914)
        (field (name Footprint) Diode_SMD:D_SOD-123))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib Mechanical) (part MountingHole)
      (description "Mounting Hole without connection")
      (docs ~)
      (footprints
        (fp MountingHole*))
      (fields
        (field (name Reference) H)
        (field (name Value) MountingHole)))
    (libpart (lib RF_GPS) (part NEO-M8T)
      (description "GNSS Module NEO M8, VCC 2.7V to 3.6V")
      (docs https://www.u-blox.com/sites/default/files/NEO-LEA-M8T-FW3_DataSheet_%28UBX-15025193%29.pdf)
      (footprints
        (fp ublox*NEO*))
      (fields
        (field (name Reference) U)
        (field (name Value) NEO-M8T)
        (field (name Footprint) RF_GPS:ublox_NEO))
      (pins
        (pin (num 1) (name TP2/~SAFEBOOT) (type BiDi))
        (pin (num 2) (name D_SEL) (type input))
        (pin (num 3) (name TIMEPULSE) (type output))
        (pin (num 4) (name EXTINT0) (type input))
        (pin (num 5) (name USB_DM) (type BiDi))
        (pin (num 6) (name USB_DP) (type BiDi))
        (pin (num 7) (name VDD_USB) (type power_in))
        (pin (num 8) (name ~RESET) (type input))
        (pin (num 9) (name VCC_RF) (type power_out))
        (pin (num 10) (name GND) (type power_in))
        (pin (num 11) (name RF_IN) (type input))
        (pin (num 12) (name GND) (type passive))
        (pin (num 13) (name GND) (type passive))
        (pin (num 14) (name LNA_EN) (type output))
        (pin (num 15) (name EXTINT1) (type input))
        (pin (num 16) (name RESERVED) (type NotConnected))
        (pin (num 17) (name RESERVED) (type NotConnected))
        (pin (num 18) (name SDA/~SPI_CS) (type BiDi))
        (pin (num 19) (name SCL/SPI_CLK) (type input))
        (pin (num 20) (name TXD/SPI_MISO) (type output))
        (pin (num 21) (name RXD/SPI_MOSI) (type input))
        (pin (num 22) (name V_BCKP) (type power_in))
        (pin (num 23) (name VCC) (type power_in))
        (pin (num 24) (name GND) (type passive))))
    (libpart (lib Regulator_Linear) (part LM1117-1.8)
      (aliases
        (alias LM1117-2.5)
        (alias LM1117-3.3)
        (alias LM1117-5.0)
        (alias TLV1117-15)
        (alias TLV1117-18)
        (alias TLV1117-25)
        (alias TLV1117-33)
        (alias TLV1117-50))
      (description "800mA Low-Dropout Linear Regulator, 1.8V fixed output, TO-220/TO-252/TO-263/SOT-223")
      (docs http://www.ti.com/lit/ds/symlink/lm1117.pdf)
      (footprints
        (fp SOT?223*)
        (fp TO?263*)
        (fp TO?252*)
        (fp TO?220*))
      (fields
        (field (name Reference) U)
        (field (name Value) LM1117-1.8))
      (pins
        (pin (num 1) (name GND) (type power_in))
        (pin (num 2) (name VO) (type power_out))
        (pin (num 3) (name VI) (type power_in))))
    (libpart (lib Sensor_Temperature) (part DS18B20U)
      (description "Programmable Resolution 1-Wire Digital Thermometer MSOP-8")
      (docs http://datasheets.maximintegrated.com/en/ds/DS18B20.pdf)
      (footprints
        (fp MSOP*3x3mm*P0.65mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) DS18B20U)
        (field (name Footprint) Package_SO:MSOP-8_3x3mm_P0.65mm))
      (pins
        (pin (num 1) (name DQ) (type BiDi))
        (pin (num 2) (name NC) (type NotConnected))
        (pin (num 3) (name NC) (type NotConnected))
        (pin (num 4) (name GND) (type power_in))
        (pin (num 5) (name NC) (type NotConnected))
        (pin (num 6) (name NC) (type NotConnected))
        (pin (num 7) (name NC) (type NotConnected))
        (pin (num 8) (name VDD) (type power_in))))
    (libpart (lib Switch) (part SW_Push)
      (description "Push button switch, generic, two pins")
      (docs ~)
      (fields
        (field (name Reference) SW)
        (field (name Value) SW_Push))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive)))))
  (libraries
    (library (logical Connector)
      (uri /usr/local/share/kicad/library/Connector.lib))
    (library (logical Connector_Generic)
      (uri /usr/local/share/kicad/library/Connector_Generic.lib))
    (library (logical Device)
      (uri /usr/local/share/kicad/library/Device.lib))
    (library (logical Diode)
      (uri /usr/local/share/kicad/library/Diode.lib))
    (library (logical Mechanical)
      (uri /usr/local/share/kicad/library/Mechanical.lib))
    (library (logical RF_GPS)
      (uri /usr/local/share/kicad/library/RF_GPS.lib))
    (library (logical Regulator_Linear)
      (uri /usr/local/share/kicad/library/Regulator_Linear.lib))
    (library (logical Sensor_Temperature)
      (uri /usr/local/share/kicad/library/Sensor_Temperature.lib))
    (library (logical Switch)
      (uri /usr/local/share/kicad/library/Switch.lib)))
  (nets
    (net (code 1) (name GND)
      (node (ref U3) (pin 12))
      (node (ref U3) (pin 13))
      (node (ref U3) (pin 24))
      (node (ref U2) (pin 1))
      (node (ref J1) (pin 39))
      (node (ref J2) (pin 9))
      (node (ref U3) (pin 10))
      (node (ref C6) (pin 2))
      (node (ref J6) (pin 2))
      (node (ref C3) (pin 2))
      (node (ref R5) (pin 2))
      (node (ref J4) (pin 2))
      (node (ref BT1) (pin 2))
      (node (ref J5) (pin 5))
      (node (ref J5) (pin 6))
      (node (ref C1) (pin 2))
      (node (ref U1) (pin 4))
      (node (ref R1) (pin 2))
      (node (ref U4) (pin 1))
      (node (ref C4) (pin 2))
      (node (ref SW1) (pin 1))
      (node (ref C5) (pin 2))
      (node (ref J2) (pin 10)))
    (net (code 2) (name +5V)
      (node (ref J1) (pin 2))
      (node (ref D1) (pin 2)))
    (net (code 3) (name "Net-(J3-Pad3)")
      (node (ref J4) (pin 1))
      (node (ref J3) (pin 3)))
    (net (code 4) (name "Net-(J3-Pad2)")
      (node (ref J3) (pin 2))
      (node (ref R2) (pin 1)))
    (net (code 5) (name "Net-(J3-Pad1)")
      (node (ref U3) (pin 9))
      (node (ref J3) (pin 1)))
    (net (code 6) (name "Net-(J6-Pad1)")
      (node (ref U3) (pin 11))
      (node (ref J6) (pin 1))
      (node (ref L1) (pin 2)))
    (net (code 7) (name /1WIRE)
      (node (ref J2) (pin 7))
      (node (ref U1) (pin 1)))
    (net (code 8) (name "Net-(J1-Pad38)")
      (node (ref J1) (pin 38))
      (node (ref J2) (pin 4)))
    (net (code 9) (name "Net-(J1-Pad40)")
      (node (ref J1) (pin 40))
      (node (ref J2) (pin 2)))
    (net (code 10) (name "Net-(J1-Pad37)")
      (node (ref J2) (pin 6))
      (node (ref J1) (pin 37)))
    (net (code 11) (name "Net-(SW1-Pad2)")
      (node (ref U3) (pin 8))
      (node (ref SW1) (pin 2)))
    (net (code 12) (name "Net-(J5-Pad2)")
      (node (ref R4) (pin 1))
      (node (ref J5) (pin 2)))
    (net (code 13) (name "Net-(J5-Pad3)")
      (node (ref R3) (pin 1))
      (node (ref J5) (pin 3)))
    (net (code 14) (name "Net-(R4-Pad2)")
      (node (ref U3) (pin 5))
      (node (ref R4) (pin 2)))
    (net (code 15) (name "Net-(R3-Pad2)")
      (node (ref U3) (pin 6))
      (node (ref R3) (pin 2)))
    (net (code 16) (name "Net-(C3-Pad1)")
      (node (ref R2) (pin 2))
      (node (ref L1) (pin 1))
      (node (ref C3) (pin 1)))
    (net (code 17) (name "Net-(J1-Pad12)")
      (node (ref J2) (pin 8))
      (node (ref J1) (pin 12)))
    (net (code 18) (name "Net-(U3-Pad14)")
      (node (ref U3) (pin 14)))
    (net (code 19) (name "Net-(J5-Pad4)")
      (node (ref J5) (pin 4)))
    (net (code 20) (name "Net-(BT1-Pad1)")
      (node (ref BT1) (pin 1))
      (node (ref U3) (pin 22)))
    (net (code 21) (name "Net-(U3-Pad18)")
      (node (ref U3) (pin 18)))
    (net (code 22) (name "Net-(J1-Pad36)")
      (node (ref J1) (pin 36)))
    (net (code 23) (name "Net-(J1-Pad34)")
      (node (ref J1) (pin 34)))
    (net (code 24) (name "Net-(J1-Pad32)")
      (node (ref J1) (pin 32)))
    (net (code 25) (name "Net-(J1-Pad30)")
      (node (ref J1) (pin 30)))
    (net (code 26) (name "Net-(J1-Pad28)")
      (node (ref J1) (pin 28)))
    (net (code 27) (name "Net-(J1-Pad26)")
      (node (ref J1) (pin 26)))
    (net (code 28) (name "Net-(J1-Pad24)")
      (node (ref J1) (pin 24)))
    (net (code 29) (name "Net-(J1-Pad22)")
      (node (ref J1) (pin 22)))
    (net (code 30) (name "Net-(J1-Pad20)")
      (node (ref J1) (pin 20)))
    (net (code 31) (name "Net-(J1-Pad18)")
      (node (ref J1) (pin 18)))
    (net (code 32) (name "Net-(U3-Pad2)")
      (node (ref U3) (pin 2)))
    (net (code 33) (name "Net-(U3-Pad1)")
      (node (ref U3) (pin 1)))
    (net (code 34) (name "Net-(U3-Pad4)")
      (node (ref U3) (pin 4)))
    (net (code 35) (name "Net-(U3-Pad15)")
      (node (ref U3) (pin 15)))
    (net (code 36) (name "Net-(U3-Pad19)")
      (node (ref U3) (pin 19)))
    (net (code 37) (name "Net-(J1-Pad7)")
      (node (ref J1) (pin 7)))
    (net (code 38) (name "Net-(J1-Pad5)")
      (node (ref J1) (pin 5)))
    (net (code 39) (name "Net-(J1-Pad3)")
      (node (ref J1) (pin 3)))
    (net (code 40) (name "Net-(J1-Pad1)")
      (node (ref J1) (pin 1)))
    (net (code 41) (name "Net-(C1-Pad1)")
      (node (ref D1) (pin 1))
      (node (ref C1) (pin 1))
      (node (ref U2) (pin 3)))
    (net (code 42) (name "Net-(J1-Pad9)")
      (node (ref J1) (pin 9)))
    (net (code 43) (name "Net-(J1-Pad29)")
      (node (ref J1) (pin 29)))
    (net (code 44) (name "Net-(J1-Pad16)")
      (node (ref J1) (pin 16)))
    (net (code 45) (name "Net-(J1-Pad14)")
      (node (ref J1) (pin 14)))
    (net (code 46) (name "Net-(J1-Pad10)")
      (node (ref J1) (pin 10)))
    (net (code 47) (name "Net-(J1-Pad8)")
      (node (ref J1) (pin 8)))
    (net (code 48) (name "Net-(J1-Pad6)")
      (node (ref J1) (pin 6)))
    (net (code 49) (name "Net-(J1-Pad4)")
      (node (ref J1) (pin 4)))
    (net (code 50) (name "Net-(J1-Pad35)")
      (node (ref J1) (pin 35)))
    (net (code 51) (name "Net-(J1-Pad33)")
      (node (ref J1) (pin 33)))
    (net (code 52) (name "Net-(J1-Pad31)")
      (node (ref J1) (pin 31)))
    (net (code 53) (name "Net-(J1-Pad27)")
      (node (ref J1) (pin 27)))
    (net (code 54) (name "Net-(J1-Pad25)")
      (node (ref J1) (pin 25)))
    (net (code 55) (name "Net-(J1-Pad23)")
      (node (ref J1) (pin 23)))
    (net (code 56) (name "Net-(J1-Pad21)")
      (node (ref J1) (pin 21)))
    (net (code 57) (name "Net-(J1-Pad19)")
      (node (ref J1) (pin 19)))
    (net (code 58) (name "Net-(J1-Pad17)")
      (node (ref J1) (pin 17)))
    (net (code 59) (name "Net-(J1-Pad15)")
      (node (ref J1) (pin 15)))
    (net (code 60) (name "Net-(J1-Pad13)")
      (node (ref J1) (pin 13)))
    (net (code 61) (name "Net-(J1-Pad11)")
      (node (ref J1) (pin 11)))
    (net (code 62) (name /GPS_PPS)
      (node (ref U3) (pin 3))
      (node (ref J2) (pin 5)))
    (net (code 63) (name +3V3)
      (node (ref U2) (pin 2))
      (node (ref C2) (pin 1))
      (node (ref C6) (pin 1))
      (node (ref U1) (pin 8))
      (node (ref U3) (pin 23)))
    (net (code 64) (name /GPS_RX)
      (node (ref U3) (pin 21))
      (node (ref J2) (pin 3)))
    (net (code 65) (name /GPS_TX)
      (node (ref J2) (pin 1))
      (node (ref U3) (pin 20)))
    (net (code 66) (name "Net-(U3-Pad17)")
      (node (ref U3) (pin 17)))
    (net (code 67) (name "Net-(U3-Pad16)")
      (node (ref U3) (pin 16)))
    (net (code 68) (name "Net-(U1-Pad7)")
      (node (ref U1) (pin 7)))
    (net (code 69) (name "Net-(U1-Pad6)")
      (node (ref U1) (pin 6)))
    (net (code 70) (name "Net-(U1-Pad5)")
      (node (ref U1) (pin 5)))
    (net (code 71) (name "Net-(U1-Pad3)")
      (node (ref U1) (pin 3)))
    (net (code 72) (name "Net-(U1-Pad2)")
      (node (ref U1) (pin 2)))
    (net (code 73) (name "Net-(C5-Pad1)")
      (node (ref C5) (pin 1))
      (node (ref U4) (pin 3))
      (node (ref J5) (pin 1)))
    (net (code 74) (name "Net-(C2-Pad2)")
      (node (ref C2) (pin 2))
      (node (ref R1) (pin 1)))
    (net (code 75) (name "Net-(R5-Pad1)")
      (node (ref R6) (pin 1))
      (node (ref U4) (pin 2))
      (node (ref U3) (pin 7))
      (node (ref R5) (pin 1)))
    (net (code 76) (name "Net-(C4-Pad1)")
      (node (ref C4) (pin 1))
      (node (ref R6) (pin 2)))))