(footprint "Crystal_SMD_5032-10Pin_5.0x3.2mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -2.8 0)
		(layer "F.SilkS")
		(uuid "fb413243-d2ac-4262-ab43-f9fd1e37fb2c")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "Crystal_SMD_5032-10Pin_5.0x3.2mm"
		(at 0 2.8 0)
		(layer "F.Fab")
		(uuid "9750a7bd-fe65-4167-ba1e-c15d06801ad7")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "5bbb5482-6e23-4bb3-bfbe-918447288a65")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "53c75701-f896-4c28-a402-52213fc93a4d")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -2.76 -1.86)
		(end -2.71 -1.86)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "56019a6c-ff88-4c10-bd36-17ffea2d8819")
	)
	(fp_line
		(start -2.76 1.86)
		(end -2.76 -1.86)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "c5a3dacc-9735-478f-b5b0-2c7d25f076be")
	)
	(fp_line
		(start -2.71 1.86)
		(end -2.76 1.86)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "d8a0bf13-021d-49d6-a8a3-df2fefa00bb5")
	)
	(fp_line
		(start -2.71 2.21)
		(end -2.71 1.86)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "7be0319e-1095-4d8b-884d-179201eeb2bc")
	)
	(fp_line
		(start -0.59 -1.86)
		(end 0.59 -1.86)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "f23dfc84-9d36-42e5-a7b8-dcc355e6aaeb")
	)
	(fp_line
		(start -0.59 1.86)
		(end -0.59 2.21)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "046a3061-9cc8-4a81-ae85-bf37fef84e58")
	)
	(fp_line
		(start 0.59 1.86)
		(end -0.59 1.86)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "35787daf-996a-4038-a6ff-759a8abde035")
	)
	(fp_line
		(start 2.71 -1.86)
		(end 2.76 -1.86)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "069e9547-886a-41b3-b121-7ad39a6af06f")
	)
	(fp_line
		(start 2.76 -1.86)
		(end 2.76 1.86)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "643cb379-90b4-447c-addf-543a0b5844cc")
	)
	(fp_line
		(start 2.76 1.86)
		(end 2.71 1.86)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "a380fac9-9ccb-41d2-8f9f-4161cd76acc3")
	)
	(fp_rect
		(start -3 -2.1)
		(end 3 2.1)
		(stroke
			(width 0.05)
			(type solid)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "372f156c-5243-4f0c-8a34-268d009833c9")
	)
	(fp_poly
		(pts
			(xy -2.5 -1.6) (xy -2.5 0.8) (xy -1.7 1.6) (xy 2.5 1.6) (xy 2.5 -1.6)
		)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill no)
		(layer "F.Fab")
		(uuid "49609857-d6fc-46c9-8259-2465c9dbfa27")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "184f9df6-675e-42b8-aa7e-8786dbb267a7")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd roundrect
		(at -1.925 1.15)
		(size 1.35 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(thermal_bridge_angle 45)
		(uuid "1457931b-bef3-4e9e-99c6-15136865de0e")
	)
	(pad "2" smd roundrect
		(at -0.6 0.975)
		(size 0.7 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(thermal_bridge_angle 45)
		(uuid "8f02f911-ea75-4b6d-b8ce-06e94f183567")
	)
	(pad "3" smd roundrect
		(at 0.6 0.975)
		(size 0.7 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(thermal_bridge_angle 45)
		(uuid "3b39c3f1-c015-44c3-ab52-f3eee930358e")
	)
	(pad "4" smd roundrect
		(at 1.925 1.15)
		(size 1.35 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(thermal_bridge_angle 45)
		(uuid "4f6d9c17-d417-48f5-84f3-69bcbd29f0ca")
	)
	(pad "5" smd roundrect
		(at 1.925 0 90)
		(size 0.7 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(thermal_bridge_angle 45)
		(uuid "6a51d1dd-dcd8-4efd-8e80-7ce563203b33")
	)
	(pad "6" smd roundrect
		(at 1.925 -1.15)
		(size 1.35 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(thermal_bridge_angle 45)
		(uuid "07be3ced-de91-4acf-bbb5-68b53d04cc8f")
	)
	(pad "7" smd roundrect
		(at 0.6 -0.975)
		(size 0.7 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(thermal_bridge_angle 45)
		(uuid "e72ac495-f4af-42f4-a82d-3a6d3a5e162d")
	)
	(pad "8" smd roundrect
		(at -0.6 -0.975)
		(size 0.7 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(thermal_bridge_angle 45)
		(uuid "f8a30606-a333-4108-8fbb-06f47740d1f1")
	)
	(pad "9" smd roundrect
		(at -1.925 -1.15)
		(size 1.35 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(thermal_bridge_angle 45)
		(uuid "bbae0aef-d483-403c-814b-d8eace04f64b")
	)
	(pad "10" smd roundrect
		(at -1.925 0 90)
		(size 0.7 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(thermal_bridge_angle 45)
		(uuid "be7bf80f-75c1-44ec-9bbc-4b9b400a8556")
	)
	(embedded_fonts no)
	(model "${KIPRJMOD}/shapes3d/Ceramic_5032_10pins.STEP"
		(offset
			(xyz 0 0 0.7)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -0 -90 -0)
		)
	)
)
