(footprint "MouseBites-5mm" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 61DD5A76)
  (fp_text reference "REF**" (at 4 -4 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 4045831e-2a8c-4c83-9815-ea4fe6f198ba)
  )
  (fp_text value "MouseBites-5mm" (at 0 1 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp fa24fc40-7c81-4fb1-afac-56db7c6b4325)
  )
  (pad "" np_thru_hole circle (at 0 1) (size 0.8 0.8) (drill 0.8) (layers F&B.Cu) (tstamp 1c301ecd-c589-4b4d-9705-26b36bce9b83))
  (pad "" np_thru_hole circle (at 0 -1) (size 0.8 0.8) (drill 0.8) (layers F&B.Cu) (tstamp 3d975253-17a3-4c62-b041-a4f126f9ea4b))
  (pad "" np_thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.8) (layers F&B.Cu) (tstamp 8d9aeddd-ad16-434f-810f-cce2475a9ff0))
  (pad "" np_thru_hole circle (at 0 2) (size 0.8 0.8) (drill 0.8) (layers F&B.Cu) (tstamp c88e73e2-fa68-49bb-a894-71173f1d206c))
  (pad "" np_thru_hole circle (at 0 -2) (size 0.8 0.8) (drill 0.8) (layers F&B.Cu) (tstamp e7ac7ed6-0073-4c2d-a197-29ae450618b4))
)
