(footprint "DFN-6-1EP_2x2mm_P0.65mm_EP0.6x1.37mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "DFN, 6 Pin (https://www.diodes.com/assets/Package-Files/U-DFN2020-6%20(Type%20C).pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
	(tags "DFN NoLead")
	(property "Reference" "REF**"
		(at 0 -1.95 0)
		(layer "F.SilkS")
		(uuid "3a847146-07d3-4259-822b-8207b9e67c28")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "DFN-6-1EP_2x2mm_P0.65mm_EP0.6x1.37mm"
		(at 0 1.95 0)
		(layer "F.Fab")
		(uuid "e02f4068-2bba-485a-8d82-678c76ccc4e0")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "b87d72bd-cdce-410d-a793-0389cd80845f")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "935aa1e5-90ec-4cc5-9229-9c95ec5988db")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -1.11 1.11)
		(end -1.11 1.06)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "ed6b2b52-fff0-4aeb-b8ff-8706d83e58cc")
	)
	(fp_line
		(start -0.925042 -1.11)
		(end 1.11 -1.11)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "090cf12b-305a-458e-9bdc-7669f3b38df1")
	)
	(fp_line
		(start 1.11 -1.11)
		(end 1.11 -1.06)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "96a4a88c-83d5-4945-9817-618cc3412813")
	)
	(fp_line
		(start 1.11 1.06)
		(end 1.11 1.11)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "0f4c8d0f-a2e6-4411-b332-083fa82eba01")
	)
	(fp_line
		(start 1.11 1.11)
		(end -1.11 1.11)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "990aaf40-42b8-488d-bcd6-bf65f25049a2")
	)
	(fp_poly
		(pts
			(xy -1.26 -1.06) (xy -1.4 -1.25) (xy -1.12 -1.25)
		)
		(stroke
			(width 0.12)
			(type solid)
		)
		(fill yes)
		(layer "F.SilkS")
		(uuid "329652a3-1689-43c3-9f9a-f16a08215e11")
	)
	(fp_line
		(start -1.6 -1.05)
		(end -1.25 -1.05)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "113f4b0d-25b3-4c9f-af49-031cf1cab92b")
	)
	(fp_line
		(start -1.6 1.05)
		(end -1.6 -1.05)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "3a9de090-d86a-41eb-b662-42f7b41e307e")
	)
	(fp_line
		(start -1.25 -1.25)
		(end 1.25 -1.25)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "994df4f5-48bc-4d14-a793-9c7c9994029c")
	)
	(fp_line
		(start -1.25 -1.05)
		(end -1.25 -1.25)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "d0141ed3-bb33-4d8d-923c-bc3bd7039ef5")
	)
	(fp_line
		(start -1.25 1.05)
		(end -1.6 1.05)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "2b28bb1a-a385-4906-8938-a20fe24e7fb6")
	)
	(fp_line
		(start -1.25 1.25)
		(end -1.25 1.05)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "59397485-6a61-408d-89aa-de9974e88f5f")
	)
	(fp_line
		(start 1.25 -1.25)
		(end 1.25 -1.05)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "7ad76c26-c525-41f3-9a0d-2065a6035201")
	)
	(fp_line
		(start 1.25 -1.05)
		(end 1.6 -1.05)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "ecd5e5b6-3252-4153-badd-f66dc9c99f15")
	)
	(fp_line
		(start 1.25 1.05)
		(end 1.25 1.25)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "876bd629-b0aa-49d5-b616-718eeda391ca")
	)
	(fp_line
		(start 1.25 1.25)
		(end -1.25 1.25)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "a93802d4-aff5-4f39-8ccd-5fdf4aebe25f")
	)
	(fp_line
		(start 1.6 -1.05)
		(end 1.6 1.05)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "12a03192-33f6-4380-a4d9-8c5ae38ab032")
	)
	(fp_line
		(start 1.6 1.05)
		(end 1.25 1.05)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "10a6e8c2-cc22-4aab-bdfb-85db98f912cc")
	)
	(fp_poly
		(pts
			(xy -1 -0.5) (xy -1 1) (xy 1 1) (xy 1 -1) (xy -0.5 -1)
		)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill no)
		(layer "F.Fab")
		(uuid "a2941dab-f816-4f41-89dd-b865eff7a883")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "aa18be2f-d0a1-44d1-8669-54274aa173c4")
		(effects
			(font
				(size 0.5 0.5)
				(thickness 0.08)
			)
		)
	)
	(pad "" smd roundrect
		(at 0 -0.325)
		(size 0.4 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "37e25d74-591e-49e9-924e-4519eaf540d4")
	)
	(pad "" smd roundrect
		(at 0 0.325)
		(size 0.4 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "7004156b-4647-4bef-924a-7ed6a81db882")
	)
	(pad "1" smd roundrect
		(at -0.925 -0.65)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "bdde3a8d-8d33-4937-b0ad-0d50e86ccb8c")
	)
	(pad "2" smd roundrect
		(at -0.925 0)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "dd9083dc-d20f-4a14-b0f9-0697aea1b0b7")
	)
	(pad "3" smd roundrect
		(at -0.925 0.65)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "dbad49e6-e04c-4d00-8076-80f33204e2ae")
	)
	(pad "4" smd roundrect
		(at 0.925 0.65)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "c641c7a6-bd7d-405a-9515-62ad178df088")
	)
	(pad "5" smd roundrect
		(at 0.925 0)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "e27e4065-c41b-4607-a09b-467fab78503e")
	)
	(pad "6" smd roundrect
		(at 0.925 -0.65)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "a4ef7aa4-d314-4065-83f7-4a5c6759b350")
	)
	(pad "7" smd roundrect
		(at 0 0)
		(size 0.6 1.37)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(chamfer_ratio 0.33)
		(chamfer top_left)
		(zone_connect 2)
		(uuid "e517a4b1-f447-439a-8031-faec2a576488")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/DFN-6-1EP_2x2mm_P0.65mm_EP1x1.6mm.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
