(footprint "RJ45_Hanrun_HR911130A_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "1 Port RJ45 8P8C receptacle, shielded, with magnetics, through hole, 2 LEDs, tab down, http://www.hanrun.com/public/upload/down/2020/09-11/cc11be56d66bb63d5f1eeb85492439c0.pdf")
	(tags "RJ45 Magjack ethernet")
	(property "Reference" "REF**"
		(at 0 11.36 180)
		(layer "F.SilkS")
		(uuid "52ee1736-ce5d-46c6-a5b2-1e50bd721285")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "RJ45_Hanrun_HR911130A_Horizontal"
		(at 4.44 11.86 0)
		(layer "F.Fab")
		(uuid "2a234c9b-1fe2-448b-9a78-15320e1a25a8")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "987d3197-8215-4739-bc2c-13047c747c75")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "fd777f5a-418c-45a4-b734-6dee37fdb85b")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start -8.13 1.43)
		(end -8.13 -5.59)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "ab7c113a-280a-4f9a-bbd8-2a59c79348ed")
	)
	(fp_line
		(start -8.13 10.51)
		(end -8.13 4.71)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "bd96601a-6c15-4c03-9dcc-93e2b8242b99")
	)
	(fp_line
		(start 8.13 1.43)
		(end 8.13 -5.59)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "a20a5ff1-6bf2-481c-b7e5-7e3bfc36c24c")
	)
	(fp_line
		(start 8.13 10.51)
		(end -8.13 10.51)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "33b6ad0c-7767-4ea0-b826-5c4d272aa9e0")
	)
	(fp_line
		(start 8.13 10.51)
		(end 8.13 4.71)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "53b7ead2-a066-463a-96bf-4ca8974de222")
	)
	(fp_line
		(start 8.36 7.26)
		(end 8.36 5.46)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "7ac4a073-8d81-4603-b850-d5a303460f3a")
	)
	(fp_line
		(start -9.5 2.31)
		(end -9.5 3.79)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "70d5e57c-fa2c-47f4-a0ce-c8be4207c5ec")
	)
	(fp_line
		(start -9.5 2.31)
		(end -8.52 1.33)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "7b494af4-8aa3-435d-8418-6936e58b4e7e")
	)
	(fp_line
		(start -9.5 3.79)
		(end -8.52 4.77)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "97b8351a-d982-46a3-933e-9b2bb929d3e9")
	)
	(fp_line
		(start -8.52 1.33)
		(end -8.52 -11.4)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "281b69a5-2c77-4b11-a4a2-ab2de929ed2a")
	)
	(fp_line
		(start -8.52 10.9)
		(end -8.52 4.77)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "74212fb9-ef00-463e-b703-a27dfabdcd9f")
	)
	(fp_line
		(start 8.52 -11.4)
		(end -8.52 -11.4)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "1ba9fc8f-d04e-44c7-9354-640aa8dfc49e")
	)
	(fp_line
		(start 8.52 1.33)
		(end 8.52 -11.4)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "5398fa6a-ee79-4a70-aebe-07b855f6ecac")
	)
	(fp_line
		(start 8.52 10.9)
		(end -8.52 10.9)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "842f528a-2541-41ea-974b-91b48bd2f83e")
	)
	(fp_line
		(start 8.52 10.9)
		(end 8.52 4.77)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "ae1cfe9a-723d-44f9-a592-5e9ecb79ef27")
	)
	(fp_line
		(start 9.5 2.31)
		(end 8.52 1.33)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "17ea85c7-7890-478c-97d2-68aa3008f339")
	)
	(fp_line
		(start 9.5 3.79)
		(end 8.52 4.77)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "86f46502-9294-4191-bed6-11814a6f4edf")
	)
	(fp_line
		(start 9.5 3.79)
		(end 9.5 2.31)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "646dd0b5-ce69-4dcd-8d2f-badd70613321")
	)
	(fp_line
		(start -8.02 10.4)
		(end -8.02 -10.9)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "f895e20e-759d-46bb-8daf-f4cb94609b84")
	)
	(fp_line
		(start 7.02 6.37)
		(end 8.02 5.37)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "6bed8b79-95aa-499f-bda7-883a354598eb")
	)
	(fp_line
		(start 7.02 6.37)
		(end 8.02 7.37)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "eb0cfb1c-bd86-42f9-a83a-338e0c91634f")
	)
	(fp_line
		(start 8.02 -10.9)
		(end -8.02 -10.9)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "15f8c3ca-6502-455f-bcc2-b60059a72e7a")
	)
	(fp_line
		(start 8.02 5.37)
		(end 8.02 -10.9)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "b82fbde3-32e0-432a-8e47-4fa981dc3739")
	)
	(fp_line
		(start 8.02 10.4)
		(end -8.02 10.4)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "a7b32d4d-7c66-4970-aa27-f144c530451c")
	)
	(fp_line
		(start 8.02 10.4)
		(end 8.02 7.37)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "0b022c12-c5c2-47e3-bd55-e1f27f9d09ad")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 180)
		(layer "F.Fab")
		(uuid "ab0934c5-81df-4201-b195-a63d277dd41c")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "" np_thru_hole circle
		(at -5.715 0 180)
		(size 3.25 3.25)
		(drill 3.25)
		(layers "*.Cu" "*.Mask")
		(uuid "3626b909-2a2e-4297-a8a5-b7d3020bea81")
	)
	(pad "" np_thru_hole circle
		(at 5.715 0 180)
		(size 3.25 3.25)
		(drill 3.25)
		(layers "*.Cu" "*.Mask")
		(uuid "c874b83d-dcaf-4719-a1c4-7d292155ef59")
	)
	(pad "P1" thru_hole roundrect
		(at 6 8.89)
		(size 1.5 1.5)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.1666666667)
		(uuid "881b690e-04bd-41c7-98c1-b676d4e0e38e")
	)
	(pad "P2" thru_hole circle
		(at 4.44 6.35)
		(size 1.5 1.5)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "31aadaa4-d482-4183-a2b4-db659767b95f")
	)
	(pad "P3" thru_hole circle
		(at 3.18 8.89)
		(size 1.5 1.5)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "2f2b035c-c7a2-45cc-b5a5-55b7d8c938f0")
	)
	(pad "P4" thru_hole circle
		(at 1.9 6.35)
		(size 1.5 1.5)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "f49da26f-0c26-4c14-97b1-12a5c0386d68")
	)
	(pad "P5" thru_hole circle
		(at 0.64 8.89)
		(size 1.5 1.5)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "cf16e346-7eb0-4450-a5b3-c9d865095636")
	)
	(pad "P6" thru_hole circle
		(at -0.64 6.35)
		(size 1.5 1.5)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "449f88de-faac-4135-a52f-79911a6024a1")
	)
	(pad "P7" thru_hole circle
		(at -1.9 8.89)
		(size 1.5 1.5)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "0faf920b-33cc-48cd-a259-22b478a98577")
	)
	(pad "P8" thru_hole circle
		(at -3.18 6.35)
		(size 1.5 1.5)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "d51abd0b-16f8-4d8a-865c-c2f7e4b4dd82")
	)
	(pad "P9" thru_hole circle
		(at -4.44 8.89)
		(size 1.5 1.5)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "eaf87f6e-f564-43c7-a21c-6d06a97250ac")
	)
	(pad "P10" thru_hole circle
		(at -5.72 6.35)
		(size 1.5 1.5)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "37f0f0f8-e721-43f2-8562-4599496b919e")
	)
	(pad "P11" thru_hole circle
		(at 6.625 -4.9 180)
		(size 1.5 1.5)
		(drill 1.02)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "87c4e00b-1c9d-41e3-98c7-1befe99aa2e9")
	)
	(pad "P12" thru_hole circle
		(at 4.085 -4.9 180)
		(size 1.5 1.5)
		(drill 1.02)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "1e7fa218-88b4-4661-a218-c53e342bbf48")
	)
	(pad "P13" thru_hole circle
		(at -4.085 -4.9 180)
		(size 1.5 1.5)
		(drill 1.02)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "32e54d30-e6cb-49bc-b1cb-744fec353963")
	)
	(pad "P14" thru_hole circle
		(at -6.625 -4.9 180)
		(size 1.5 1.5)
		(drill 1.02)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "95e40be4-9e03-4812-8c78-d4e13786951d")
	)
	(pad "SH" thru_hole circle
		(at -7.745 3.05 180)
		(size 2.5 2.5)
		(drill 1.63)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "201b1c0a-5dbe-41b2-ab9e-13e21e988740")
	)
	(pad "SH" thru_hole circle
		(at 7.745 3.05 180)
		(size 2.5 2.5)
		(drill 1.63)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "20f3ee30-c6a9-47a0-a426-b1fc61d0799e")
	)
	(embedded_fonts no)
	(model "${KIPRJMOD}/shapes3d/Hanrun_HR911130A.STEP"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 -0 -180)
		)
	)
)
